**Organizer:** Street Cats Car Club **Date**: \_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_

**Driver Names (Up to two):** \_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_ \_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_

**Vehicle Model, Make, Year, Colour**: \_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_

**Vehicle Class (if unknown, please list all modifications):**

|  |  |  |  |
| --- | --- | --- | --- |
| **Safety List**  |  | **Brakes** |  |
| Helmet: FIA or SFI approved, within expiry date. |  | Brake Lights: functional. |  |
| OEM seat belts: functional and in good condition. |  | Steel and flexible lines: fittings, attachments, mounting and integrity OK. |  |
| Seats: securely mounted and in good condition. |  | 15 second static brake test: pedal firm - no loss of foot pressure. |  |
| Safety Harness (if applicable): FIA or SFI approved, within expiry date, and installed to manufacturer’s specifications. |  | Friction Materials: pads, shoes; greater than 50% of manufacturer’s thickness specifications. |  |
| Battery: securely tied down, battery box for remote battery. |  | Calipers and/or brake cylinders: no leaks, operating freely, attachment hardware secure. |  |
| **Fuel System** |  | Brake fluid: level checked and OK with minimal moisture content. |  |
| Gas tank or fuel cell: no leaks, attachment secure, filler cap and vent cap present. |  | **Steering and Suspension** |  |
| Fuel lines: in good condition, no leaks or structural corrosion. |  | Ball joints/swivel point: within wear limits, grease seals intact, attachment secure. |  |
| Fuel filter(s): clamps on flex hose, no cracks or leaks. |  | Idler arm, pitman arm, links & tie rod/link ends: within wear limits, secure attachment, seals intact. |  |
| Fuel delivery lines from tank: no leaks, secure routing. |  | Bearings: hubs properly adjusted within manufacturer’s specifications, cotter pins or locking devices secure. |  |
| Carburetor, fuel injection systems, injectors: no leaks. |  | General condition of system: springs, shocks, bushings, frame attachments, anti-sway bar mounting. |  |
| **Exhaust System** |  | **Tires and Wheels** |  |
| Flanges, hangars and brackets securely mounted. |  | Wheels and tire valves: in good visual condition with no apparent cracks. |  |
| The exhaust system must not leak at pipe flanges or joints. |  | All studs/nuts: present & fully threaded for secure attachment. |  |
| Exhaust pipe must terminate to the side or rear of the car, and noise level be within event limits. |  | Tires: no cord showing, no cuts, no interference with body throughout range of motion. |  |

Participant’s Declaration – I/We the undersigned acknowledge that at all times it is the participants’ responsibility to ensure that the car and its components and safety equipment, and the participants’ personal safety equipment, meet the regulatory safety and technical requirements of the event entered. I/We understand that our vehicle insurance is void while participating in this event.

Driver Signature(s): \_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_ \_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_